Summary: ARP table update

Description: Verify that ARP table updates after getting ARP reply

Version: ARPv1

Setup Description:

PC1 --------ethernet--------- PC2

PC1: 10. 0. 2. 4

PC2: 10. 0. 2. 15

Steps (with ER):

1. Clean ARP table

arp -d <IP of PC2>

ER: ARP table is empty

1. Run Wireshark for ethernet
2. Run ping from PC1 to PC2

ER: Ping is running

1. Verify the ARP table with arp -a command

ER: There is a record in ARP table giving us required info about IP&MAC adresses.